**How to check IP address**

1. Press on the keyboard CTRL-ALT-CANC
2. Appear a popup window called Task Manager.
3. Select “New Task”.
4. Write “cmd” and press Enter.
5. Automatically the PC open a black window of Dos. Write “ipconfig” -> press Enter.
6. The PC show you the configuration of the Network Card:

IP ADDRESS: 192.168.0.1 0-255

Subnet mask: 255.255.0.0 or

255.255.255.0

**PING Procedure** (Ethernet cable test)

1. Press CTRL-ALT-CANC
2. Appear a popup window called Task Manager.
3. Select “New Task”
4. Write “cmd” and press enter.
5. In the black window of Dos. Write “ping ip address of another pc connected in the same network.” Press Enter.
6. Good cabling is:

Byte sent 4, received 4, lost 0.

1. Example:

If i make the procedure from PC1, i write in the step 5: “ping 192.168.0.2”

If i make the procedure from PC2, i write in the step 5: “ping 192.168.0.1”

Cable to test

PC2

192.168.0.2

PC1

192.168.0.1